**Specifications of surface roughness tester**

|  |  |  |
| --- | --- | --- |
| **Parameters** | | **Descriptions** |
| Model No. | | SJ-301 |
| Type of drive unit | | Standard drive unite type |
| Measuring range | X-axis | 12.5 mm |
| Z-axis | 350 µm |
| Stylus tip material | | Diamond |
| Parameters | | Ra, Rz, Rt, Rp, Rq |